**Order №**

**TESTS OF PROTECTIVE STRUCTURES ROPS & FOPS ACCORDING TO  
EN/ISO STANDARDS**

1. **ordering party**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1 | Business name | | | |
|  | | | |
| 2 | Address: | | | |
|  | | | |
| 3 | Name and position of the authorized person to contract negotiations: | | | |
|  | | | |
| 4 | Name and position of the authorized person to technical matters: | | | |
|  | | | |
| 5 | ID №: | | TAX ID №: | |
|  | |  | |
| 6 | Telephone: | Fax: | | E-mail: |
|  |  | |  |
| 7 | Bank connection: | | Account number: | |
|  | |  | |

1. **PRODUCT**

|  |  |
| --- | --- |
| 8 | Name: |
|  |
| 9 | Make, model and type: |
|  |
| 10 | Manufacturer: |
|  |
| 11 | Address: |
|  |
| 12 | Assembly plant (if not identical to the address of manufacturer): |
|  |

1. **THE REQUIRED EN/ISO TESTS**

|  |  |
| --- | --- |
| 13 | Tests of the protective structures ROPS & TOPS |
| EN ISO 3471 – Earthmoving machinery;  ISO 8082-1&2 – Forestry machinery;  EN 15059 – Snow grooming equipment;  ISO 21299 – Powered ride-on turf care equipment;  ISO 12117-2 – Excavators of over 6 t;  EN 13531+A1, ISO 12117 – Compact excavators. |
| 14 | Tests of the protective structures FOPS |
| EN ISO 3449 – Earthmoving machinery;  ISO 8083 – Forestry machinery. |
| 15 | Tests of the protective structures OPS & OPG |
| ISO 8084 – Forestry machinery; ISO 10262 – Hydraulic excavators. |
| 16 | Belt anchorages |
| ISO 3776-2 – Tractor and agriculture machinery seats;  ISO 6683 – Earthmoving machinery. |

Drawing of assembly of protective structure or anchorages is attached to this order.

|  |  |  |
| --- | --- | --- |
|  |  |  |
| Date | *(stamp)* | Name and signature of the authorized person |